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TOOELE CITY BUILDING CODES AND DESIGN CRITERIA

BUILDING CODES:

· 2024 INTERNATIONAL BUILDING CODE (IBC) INCLUDING APPENDICES C AND J.
· 2021 INTERNATIONAL RESIDENTIAL CODE (IRC) INCLUDING APPENDICES AQ AND AE 
· 2024 INTERNATIONAL PLUMBING CODE (IPC).
· 2024 INTERNATIONAL MECHANICAL CODE (IMC).
· 2024 INTERNATIONAL FUEL GAS CODE (IFC).
· 2024 INTERNATIONAL EXISTING BUILDING CODE (IEBC).
· 2023 INTERNATIONAL ENERGY CONSERVATION CODE (IECC) USE COMMERCIAL PROVISIONS
· 2015 INTERNATIONAL ENERGY CONSERVATION CODE (IECC) USE RESIDENTIAL PROVISIONS.
· 2024 INTERNATIONAL EXISTING BUILDING CODE (IEBC).
· 2023 NATIONAL ELECTRICAL CODE (NEC).
· ICC / ANSI A117.1-2009.
· UTAH STATE AMENDMENTS AS PER TITLE 15A STATE CONSTRUCTION AND FIRE CODES ACT.

DESIGN CRITERIA:

· SNOW LOAD: 
GROUND SNOW LOAD USE UTAH STATE UNIVERSITY
                          https://www.usu.edu/utahsnowload/
ROOF LOAD DETERMINED PER CHAPTER 7 OF ASCE 7-16.
· WIND: 
IRC SECTION:  	105 MPH 3 SECOND GUST EXPOSURE C.
IBC SECTION: 	RISK CATEGORY I 95
      		RISK CATEGORY II 100
       		RISK CATEGORY III 105 (MOST COMMON)
      		RISK CATEGORY IV 110
· SESMIC ZONE: 
IRC - D1
               IBC - D
· FROST DEPTH: 
30 INCHES.
· SOIL: 
IRC ASSUMED 1500 PSF 
IBC SITE SPECIFIC GEOTECHNICAL REPORT  
· CLIMATE ZONE: 
5B
· WEATHERERING: 
SEVERE 
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